# Possible Improvements

* Problems with \_\_name\_\_ - flag when using XimeaxiQCamAPI.py. See the “import scipy.ndimage.filters” command in “BeamProfilingApplication.py”
* Option to disable the fitting totally
* Search for parts that limit the performance and try to improve those. It is observed that the performance depends on the size of the ROI.
* Use methods for optimizing the fit performance (implemented, but not connected to Application GUI)
* Introduce a “reference amplitude” displayed in the amplitude bar.